Sample 511 Multi Choice Quiz
Name: ____________________________    Date: ________________
Instructions: Choose the best answer for each question. Circle A, B, C, or D.
1. When must the OSHA 300A Summary be posted?
A. January 1 through March 31
B. February 1 through April 30
C. March 1 through May 31
D. February 15 through May 15
2. By what date must the OSHA 300A Summary be submitted?
A. January 31
B. February 15
C. March 2
D. April 30
3. What is the purpose of OSHA compliance directives?
A. To establish wage rates
B. To provide consistent enforcement
C. To replace OSHA standards
D. To reduce employer recordkeeping
4. Under the multi-employer concept, which employer creates the hazardous condition?
A. Controlling employer
B. Correcting employer
C. Creating employer
D. Exposing employer
5. In general industry, at what height does fall protection generally apply?
A. 4 feet
B. 6 feet
C. 8 feet
D. 10 feet
6. What is the maximum travel distance to a Class B fire extinguisher?
A. 25 feet
B. 50 feet
C. 75 feet
D. 100 feet
7. What is the maximum travel distance to a Class A fire extinguisher?
A. 25 feet
B. 50 feet
C. 75 feet
D. 100 feet
8. How long does an employer have to contest an OSHA violation?
A. 5 working days
B. 10 working days
C. 15 working days
D. 30 calendar days
9. What does OSHA require an employer to do with each cited violation?
A. Abate every violation
B. Contest every violation
C. Pay the penalty before correcting it
D. Close the worksite immediately
10. How long must an OSHA citation be posted?
A. 1 day
B. 3 days or until abated, whichever is longer
C. 7 days only
D. Until the next inspection
11. What are the three basic stages of an OSHA compliance inspection?
A. Plan, inspect, report
B. Open, walk, close
C. Notify, cite, collect
D. Interview, test, fine
12. Compressed air used for cleaning must be reduced to no more than:
A. 20 psi
B. 25 psi
C. 30 psi
D. 40 psi
13. An opening in a floor that is 2 inches or more is considered a:
A. Gap
B. Trench
C. Hole
D. Pit
14. Which OSHA inspection priority comes first among the items listed?
A. Complaint
B. Severe injury
C. Imminent danger
D. Programmed inspection
15. An exit area that opens to the outside is called the:
A. Exit access
B. Exit route
C. Exit discharge
D. Means of egress
16. What clearance distance is noted for compressed gas cylinders/tanks?
A. 10 feet
B. 15 feet
C. 20 feet
D. 25 feet
17. Where is the OSH Act General Duty Clause found?
A. Section 4(b)(1)
B. Section 5(a)(1)
C. Section 6(a)(2)
D. Section 11(c)(1)


18. An oxygen-deficient atmosphere contains oxygen at what level?
A. Less than 19.5% by volume
B. 19.5% to 23.5% by volume
C. More than 23.5% by volume
D. Exactly 21% by volume
19. Which organization approves and certifies respirators?
A. OSHA
B. NIOSH
C. EPA
D. ANSI
20. For voltages to ground of 50 kV or less, how far must an unqualified person remain from an unguarded energized overhead line?
A. 4 feet
B. 6 feet
C. 10 feet
D. 20 feet
21. Which part of an exit route is the travel path that leads to an exit?
A. Exit access
B. Exit
C. Exit discharge
D. Safe area
22. Who may provide powered industrial truck operator training and evaluation?
A. Any experienced operator
B. The truck manufacturer only
C. The employer or the employer's designee
D. The employee being trained
23. At least how often must a powered industrial truck operator be evaluated?
A. Every year
B. Every 3 years
C. Every 5 years
D. Only after an incident
24. Which three methods safeguard employees from machine hazards?
A. Devices, guards, and location
B. PPE, warning signs, and training only
C. Lockout, ventilation, and housekeeping
D. Alarms, labels, and inspections
25. What is the point of operation on a machine?
A. The location of the emergency stop button
B. Where the stock meets the machine
C. The area where the operator stands
D. The location of the power disconnect
26. Which publication addresses in-plant handling and storage of compressed gases?
A. NFPA 10
B. CGA Pamphlet P-1-1965
C. ANSI Z87.1
D. OSHA 300A
27. Which description correctly defines a confined space?
A. Any area below ground level
B. Any room with one doorway
C. A space large enough to enter and work, with limited entry or exit, and not designed for continuous occupancy
D. Any space that contains a hazardous material
28. An employer-designated person who identifies existing and predictable hazards and has authority to correct them is a:
A. Competent person
B. Authorized employee
C. Safety committee member
D. Controlling employer
29. What must an employer perform to properly select personal protective equipment?
A. A job rotation plan
B. A hazard assessment
C. A medical evaluation for every employee
D. A recordkeeping audit
30. How often must employees involved in a process covered by process safety management receive refresher training?
A. Every year
B. Every 2 years
C. At least every 3 years
D. Every 5 years
31. What work is covered by the lockout/tagout standard?
A. Servicing and maintenance of machines and equipment
B. Routine office work
C. New-hire orientation only
D. All normal production operations
32. Under OSHA's multi-employer policy, which employer has general supervisory authority over the worksite and may have responsibility to correct hazards?
A. Creating employer
B. Exposing employer
C. Correcting employer
D. Controlling employer
33. After welding or cutting is completed, how long must a required fire watch remain?
A. 10 minutes
B. At least 30 minutes
C. 1 hour
D. Until the next shift
34. What written program is required for employees with occupational exposure to blood or other potentially infectious materials?
A. Emergency action plan
B. Hazard communication program
C. Exposure control plan
D. Respiratory protection program
35. What part of a bloodborne pathogens exposure control plan identifies job classifications and tasks in which occupational exposure may occur?
A. Exposure determination
B. Incident investigation
C. Medical surveillance
D. Return-to-work evaluation
36. How often must the employer inspect each energy-control procedure under lockout/tagout?
A. Monthly
B. At least annually
C. Every 3 years
D. Only after an injury
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